HL7 Vietnam VN Core FHIR Implementation Guide

Bộ Hướng dẫn Triển khai Core FHIR cho Việt Nam
0.5.0 - Draft for Community Review

Bộ Hướng dẫn Triển khai Core FHIR cho Việt Nam - Local Development build (v0.5.0) built by the FHIR (HL7® FHIR® Standard) Build Tools. See the Directory of published versions

## Phần mở rộng: Số lưu hành thiết bị y tế — VN Device Registration Number - Mô tả chi tiết

Draft tại thời điểm 2026-04-25

Các định nghĩa cho vn-ext-device-registration-number phần mở rộng

- Bảng phần tử chính
- Bảng Differential
- Bảng Snapshot

Guidance on how to interpret the contents of this table can be foundhere

0. Extension
Definition | Số lưu hành (registration number) của thiết bị y tế tại Việt Nam. Căn cứ pháp lý: NĐ 98/2021/NĐ-CP Điều 21 (Phân nhóm số lưu hành), Chương III (Điều 17-33) về đăng ký lưu hành TBYT, đã được sửa đổi, bổ sung bởi NĐ 07/2023/NĐ-CP (03/03/2023) và NĐ 04/2025/NĐ-CP (hiệu lực 01/01/2025). Phân nhóm theo NĐ 98/2021 Điều 21: Loại A & B — Số công bố tiêu chuẩn áp dụng (Sở Y tế tỉnh/TP tiếp nhận): Format: `[STT tiếp nhận]/[Năm tiếp nhận 2 số]/[Mã ký hiệu Sở Y tế]-PCBA` (loại A) Format: `[STT tiếp nhận]/[Năm tiếp nhận 2 số]/[Mã ký hiệu Sở Y tế]-PCBB` (loại B) PCBA/PCBB = Phiếu công bố loại A / loại B Ví dụ: `2300001/23/HN-PCBA` (Hồ sơ số 1 năm 2023, Sở Y tế Hà Nội tiếp nhận) Loại C & D — Số Giấy chứng nhận đăng ký lưu hành (Bộ Y tế cấp): Format chuẩn: `[STT cấp]/[Năm cấp 2 số]/BYT-ĐKLH` Format rút gọn: `[STT cấp]/BYT-ĐKLH` ĐKLH = Đăng ký lưu hành Ví dụ: `2300055/BYT-ĐKLH` hoặc `2300055/23/BYT-ĐKLH` Phạm vi: Bắt buộc cho loại B/C/D trước khi đưa ra thị trường Loại A chỉ công bố tiêu chuẩn áp dụng (vẫn dùng PCBA format) Đây là định danh ở mức sản phẩm/model/regulatory context, KHÔNG phải định danh per-instance Lưu ý phân biệt: Extension này độc lập với: UDI (định danh per-instance theo HL7 best practice) MA_VAT_TU (mã nghiệp vụ BHYT theo QĐ 3176) Serial number (per-instance physical) Mã tài sản BV (internal facility code) Optional Extension Element - found in all resources.
Short | Số lưu hành thiết bị y tế — VN Device Registration NumberOptional Extensions Element
Control | 0..* This element is affected by the following invariants: ele-1
Is Modifier | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
2. Extension.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | ExtensionAdditional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..0*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `Extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
4. Extension.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://fhir.hl7.org.vn/core/StructureDefinition/vn-ext-device-registration-number`
6. Extension.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Số lưu hành TBYT (PCBA/PCBB cho loại A/B, ĐKLH cho loại C/D)Value of extension
Control | 0..1
Type | Identifier, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) vn-device-regnum-format: Số lưu hành TBYT phải đúng 1 trong 3 format theo NĐ 98/2021 Điều 21: - Loại A (Sở Y tế cấp): [STT]/[Năm 2 số]/[Mã tỉnh]-PCBA — ví dụ 2300001/23/HN-PCBA - Loại B (Sở Y tế cấp): [STT]/[Năm 2 số]/[Mã tỉnh]-PCBB — ví dụ 2300002/23/HN-PCBB - Loại C/D (Bộ Y tế cấp): [STT]/[Năm 2 số]/BYT-ĐKLH hoặc [STT]/BYT-ĐKLH — ví dụ 2300055/23/BYT-ĐKLH (`value.empty() or value.matches('^\\d+/\\d{2}/[A-Z]{2,3}-PCB[AB]$') or value.matches('^\\d+(/\\d{2})?/BYT-ĐKLH$')`)
8. Extension.value[x].use
Definition | The purpose of this identifier.
Short | usual | official | temp | secondary | old (If known)
Comments | Applications can assume that an identifier is permanent unless it explicitly says that it is temporary.
Control | 0..1
Binding | The codes SHALL be taken from IdentifierUse http://hl7.org/fhir/ValueSet/identifier-use|4.0.1 (required to `http://hl7.org/fhir/ValueSet/identifier-use|4.0.1` ) Identifies the purpose for this identifier, if known .
Type | code
Is Modifier | true because This is labeled as "Is Modifier" because applications should not mistake a temporary id for a permanent one.
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Allows the appropriate identifier for a particular context of use to be selected from among a set of identifiers.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
10. Extension.value[x].system
Definition | Establishes the namespace for the value - that is, a URL that describes a set values that are unique.
Short | The namespace for the identifier value
Comments | Identifier.system is always case sensitive.
Control | 10..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | There are many sets of identifiers. To perform matching of two identifiers, we need to know what set we're dealing with. The system identifies a particular set of unique identifiers.
Fixed Value | `http://fhir.hl7.org.vn/core/sid/medical-device-registration-number`
Example | General: http://www.acme.com/identifiers/patient
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
12. Extension.value[x].value
Definition | Format theo NĐ 98/2021 Điều 21: PCBA (loại A), PCBB (loại B) do Sở Y tế cấp; ĐKLH (loại C/D) do Bộ Y tế cấp. The portion of the identifier typically relevant to the user and which is unique within the context of the system.
Short | Giá trị số lưu hànhThe value that is unique
Comments | If the value is a full URI, then the system SHALL be urn:ietf:rfc:3986. The value's primary purpose is computational mapping. As a result, it may be normalized for comparison purposes (e.g. removing non-significant whitespace, dashes, etc.) A value formatted for human display can be conveyed using the Rendered Value extension. Identifier.value is to be treated as case sensitive unless knowledge of the Identifier.system allows the processer to be confident that non-case-sensitive processing is safe.
Control | 10..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Example | General: 123456
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
14. Extension.value[x].assigner
Definition | Organization that issued/manages the identifier.
Short | Cơ quan cấp (Sở Y tế cho A/B, Bộ Y tế cho C/D)Organization that issued id (may be just text)
Comments | The Identifier.assigner may omit the .reference element and only contain a .display element reflecting the name or other textual information about the assigning organization.
Control | 0..1
Type | Reference(Organization)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))

Guidance on how to interpret the contents of this table can be foundhere

0. Extension
Definition | Số lưu hành (registration number) của thiết bị y tế tại Việt Nam. Căn cứ pháp lý: NĐ 98/2021/NĐ-CP Điều 21 (Phân nhóm số lưu hành), Chương III (Điều 17-33) về đăng ký lưu hành TBYT, đã được sửa đổi, bổ sung bởi NĐ 07/2023/NĐ-CP (03/03/2023) và NĐ 04/2025/NĐ-CP (hiệu lực 01/01/2025). Phân nhóm theo NĐ 98/2021 Điều 21: Loại A & B — Số công bố tiêu chuẩn áp dụng (Sở Y tế tỉnh/TP tiếp nhận): Format: `[STT tiếp nhận]/[Năm tiếp nhận 2 số]/[Mã ký hiệu Sở Y tế]-PCBA` (loại A) Format: `[STT tiếp nhận]/[Năm tiếp nhận 2 số]/[Mã ký hiệu Sở Y tế]-PCBB` (loại B) PCBA/PCBB = Phiếu công bố loại A / loại B Ví dụ: `2300001/23/HN-PCBA` (Hồ sơ số 1 năm 2023, Sở Y tế Hà Nội tiếp nhận) Loại C & D — Số Giấy chứng nhận đăng ký lưu hành (Bộ Y tế cấp): Format chuẩn: `[STT cấp]/[Năm cấp 2 số]/BYT-ĐKLH` Format rút gọn: `[STT cấp]/BYT-ĐKLH` ĐKLH = Đăng ký lưu hành Ví dụ: `2300055/BYT-ĐKLH` hoặc `2300055/23/BYT-ĐKLH` Phạm vi: Bắt buộc cho loại B/C/D trước khi đưa ra thị trường Loại A chỉ công bố tiêu chuẩn áp dụng (vẫn dùng PCBA format) Đây là định danh ở mức sản phẩm/model/regulatory context, KHÔNG phải định danh per-instance Lưu ý phân biệt: Extension này độc lập với: UDI (định danh per-instance theo HL7 best practice) MA_VAT_TU (mã nghiệp vụ BHYT theo QĐ 3176) Serial number (per-instance physical) Mã tài sản BV (internal facility code)
Short | Số lưu hành thiết bị y tế — VN Device Registration Number
2. Extension.extension
Control | 0..0
4. Extension.url
Fixed Value | `http://fhir.hl7.org.vn/core/StructureDefinition/vn-ext-device-registration-number`
6. Extension.value[x]
Short | Số lưu hành TBYT (PCBA/PCBB cho loại A/B, ĐKLH cho loại C/D)
Type | Identifier, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, boolean, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Invariants | vn-device-regnum-format: Số lưu hành TBYT phải đúng 1 trong 3 format theo NĐ 98/2021 Điều 21: - Loại A (Sở Y tế cấp): [STT]/[Năm 2 số]/[Mã tỉnh]-PCBA — ví dụ 2300001/23/HN-PCBA - Loại B (Sở Y tế cấp): [STT]/[Năm 2 số]/[Mã tỉnh]-PCBB — ví dụ 2300002/23/HN-PCBB - Loại C/D (Bộ Y tế cấp): [STT]/[Năm 2 số]/BYT-ĐKLH hoặc [STT]/BYT-ĐKLH — ví dụ 2300055/23/BYT-ĐKLH (`value.empty() or value.matches('^\\d+/\\d{2}/[A-Z]{2,3}-PCB[AB]$') or value.matches('^\\d+(/\\d{2})?/BYT-ĐKLH$')`)
8. Extension.value[x].system
Control | 1..?
Fixed Value | `http://fhir.hl7.org.vn/core/sid/medical-device-registration-number`
10. Extension.value[x].value
Definition | Format theo NĐ 98/2021 Điều 21: PCBA (loại A), PCBB (loại B) do Sở Y tế cấp; ĐKLH (loại C/D) do Bộ Y tế cấp.
Short | Giá trị số lưu hành
Control | 1..?
12. Extension.value[x].assigner
Short | Cơ quan cấp (Sở Y tế cho A/B, Bộ Y tế cho C/D)

Guidance on how to interpret the contents of this table can be foundhere

0. Extension
Definition | Số lưu hành (registration number) của thiết bị y tế tại Việt Nam. Căn cứ pháp lý: NĐ 98/2021/NĐ-CP Điều 21 (Phân nhóm số lưu hành), Chương III (Điều 17-33) về đăng ký lưu hành TBYT, đã được sửa đổi, bổ sung bởi NĐ 07/2023/NĐ-CP (03/03/2023) và NĐ 04/2025/NĐ-CP (hiệu lực 01/01/2025). Phân nhóm theo NĐ 98/2021 Điều 21: Loại A & B — Số công bố tiêu chuẩn áp dụng (Sở Y tế tỉnh/TP tiếp nhận): Format: `[STT tiếp nhận]/[Năm tiếp nhận 2 số]/[Mã ký hiệu Sở Y tế]-PCBA` (loại A) Format: `[STT tiếp nhận]/[Năm tiếp nhận 2 số]/[Mã ký hiệu Sở Y tế]-PCBB` (loại B) PCBA/PCBB = Phiếu công bố loại A / loại B Ví dụ: `2300001/23/HN-PCBA` (Hồ sơ số 1 năm 2023, Sở Y tế Hà Nội tiếp nhận) Loại C & D — Số Giấy chứng nhận đăng ký lưu hành (Bộ Y tế cấp): Format chuẩn: `[STT cấp]/[Năm cấp 2 số]/BYT-ĐKLH` Format rút gọn: `[STT cấp]/BYT-ĐKLH` ĐKLH = Đăng ký lưu hành Ví dụ: `2300055/BYT-ĐKLH` hoặc `2300055/23/BYT-ĐKLH` Phạm vi: Bắt buộc cho loại B/C/D trước khi đưa ra thị trường Loại A chỉ công bố tiêu chuẩn áp dụng (vẫn dùng PCBA format) Đây là định danh ở mức sản phẩm/model/regulatory context, KHÔNG phải định danh per-instance Lưu ý phân biệt: Extension này độc lập với: UDI (định danh per-instance theo HL7 best practice) MA_VAT_TU (mã nghiệp vụ BHYT theo QĐ 3176) Serial number (per-instance physical) Mã tài sản BV (internal facility code)
Short | Số lưu hành thiết bị y tế — VN Device Registration Number
Control | 0..* This element is affected by the following invariants: ele-1
Is Modifier | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
2. Extension.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
4. Extension.extension
Definition | An Extension
Short | Extension
Control | 0..0
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Extension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
6. Extension.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://fhir.hl7.org.vn/core/StructureDefinition/vn-ext-device-registration-number`
8. Extension.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Số lưu hành TBYT (PCBA/PCBB cho loại A/B, ĐKLH cho loại C/D)
Control | 0..1
Type | Identifier
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) vn-device-regnum-format: Số lưu hành TBYT phải đúng 1 trong 3 format theo NĐ 98/2021 Điều 21: - Loại A (Sở Y tế cấp): [STT]/[Năm 2 số]/[Mã tỉnh]-PCBA — ví dụ 2300001/23/HN-PCBA - Loại B (Sở Y tế cấp): [STT]/[Năm 2 số]/[Mã tỉnh]-PCBB — ví dụ 2300002/23/HN-PCBB - Loại C/D (Bộ Y tế cấp): [STT]/[Năm 2 số]/BYT-ĐKLH hoặc [STT]/BYT-ĐKLH — ví dụ 2300055/23/BYT-ĐKLH (`value.empty() or value.matches('^\\d+/\\d{2}/[A-Z]{2,3}-PCB[AB]$') or value.matches('^\\d+(/\\d{2})?/BYT-ĐKLH$')`)
10. Extension.value[x].id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
12. Extension.value[x].extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `Extension.value[x].extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
14. Extension.value[x].use
Definition | The purpose of this identifier.
Short | usual | official | temp | secondary | old (If known)
Comments | Applications can assume that an identifier is permanent unless it explicitly says that it is temporary.
Control | 0..1
Binding | The codes SHALL be taken from IdentifierUse (required to `http://hl7.org/fhir/ValueSet/identifier-use|4.0.1` ) Identifies the purpose for this identifier, if known .
Type | code
Is Modifier | true because This is labeled as "Is Modifier" because applications should not mistake a temporary id for a permanent one.
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | Allows the appropriate identifier for a particular context of use to be selected from among a set of identifiers.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
16. Extension.value[x].type
Definition | A coded type for the identifier that can be used to determine which identifier to use for a specific purpose.
Short | Description of identifier
Comments | This element deals only with general categories of identifiers. It SHOULD not be used for codes that correspond 1..1 with the Identifier.system. Some identifiers may fall into multiple categories due to common usage. Where the system is known, a type is unnecessary because the type is always part of the system definition. However systems often need to handle identifiers where the system is not known. There is not a 1:1 relationship between type and system, since many different systems have the same type.
Control | 0..1
Binding | Unless not suitable, these codes SHALL be taken from Identifier Type Codes (extensible to `http://hl7.org/fhir/ValueSet/identifier-type|4.0.1` ) A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
Type | CodeableConcept
Is Modifier | false
Summary | true
Requirements | Allows users to make use of identifiers when the identifier system is not known.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
18. Extension.value[x].system
Definition | Establishes the namespace for the value - that is, a URL that describes a set values that are unique.
Short | The namespace for the identifier value
Comments | Identifier.system is always case sensitive.
Control | 1..1
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | There are many sets of identifiers. To perform matching of two identifiers, we need to know what set we're dealing with. The system identifies a particular set of unique identifiers.
Fixed Value | `http://fhir.hl7.org.vn/core/sid/medical-device-registration-number`
Example | General: http://www.acme.com/identifiers/patient
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
20. Extension.value[x].value
Definition | Format theo NĐ 98/2021 Điều 21: PCBA (loại A), PCBB (loại B) do Sở Y tế cấp; ĐKLH (loại C/D) do Bộ Y tế cấp.
Short | Giá trị số lưu hành
Comments | If the value is a full URI, then the system SHALL be urn:ietf:rfc:3986. The value's primary purpose is computational mapping. As a result, it may be normalized for comparison purposes (e.g. removing non-significant whitespace, dashes, etc.) A value formatted for human display can be conveyed using the Rendered Value extension. Identifier.value is to be treated as case sensitive unless knowledge of the Identifier.system allows the processer to be confident that non-case-sensitive processing is safe.
Control | 1..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Example | General: 123456
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
22. Extension.value[x].period
Definition | Time period during which identifier is/was valid for use.
Short | Time period when id is/was valid for use
Control | 0..1
Type | Period
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
24. Extension.value[x].assigner
Definition | Organization that issued/manages the identifier.
Short | Cơ quan cấp (Sở Y tế cho A/B, Bộ Y tế cho C/D)
Comments | The Identifier.assigner may omit the .reference element and only contain a .display element reflecting the name or other textual information about the assigning organization.
Control | 0..1
Type | Reference(Organization)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)